123125
Kevtris
----

Included are 8 .jed files that can be used to replace all of the PALs on the original board.
The source for them is included in /PAL source.  I dumped the two PROMs but they seem to match
the original dump, but are included anyways.

To run "decrypted" <cough> ROMs, jump the following pins:

13 -> 29
14 -> 28
15 -> 27
16 -> 26
17 -> 25
18 -> 24
19 -> 23
20 -> 22

This will bypass it and pipe the data lines straight through.

I have included an image of the sound board with most of the resistors/diodes lifted up
so you can see the designators (which are inconveniently under the parts).

There could be and probably are errors in the schematic, I didn't do a very thorough 
tracing but it should be reasonably accurate.

